{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["Service Menu","Internal Menu"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Service Menu","index":0,"n_rows":92,"n_cols":13,"rows_kept":92,"cut":false,"hidden":false,"merged":[[19,3,24,3],[54,3,59,3],[2,3,7,3],[46,3,51,3],[14,3,15,3],[16,3,17,3],[8,3,9,3],[10,3,11,3],[12,3,13,3]],"flags":["formulas_cached_only"]}
[{"$nulls":4},"Factory","GOOD","DG2IAQ","DG2IAQ","DL4CU","KM6AB","mods.dk","ON7WP","PE1OPM"]
["no.","content","description","alignment / remarks","\"HOME\"","AVERAGE","actually","default","Modify","SWR mod",null,"3 / 1.5 kHz"]
[1,"HF1RXG","CW 1.825,07","The higher, the more sensitive the RX is",128,107,100,88,141,null,118,null,88]
[2,"HF2RXG","CW 7.043,55",null,128,88.6,100,76,100,null,91,null,76]
[3,"HF3RXG","CW 21.070,00",null,128,127.4,128,102,177,null,133,null,97]
[4,"50MRXG","CW 50.095,00",null,128,124.2,128,116,174,null,106,null,97]
[5,"VHFRXG","CW 145.375,00",null,128,95,128,80,118,null,77,null,72]
[6,"UHFRXG","CW 433.425,00",null,128,108.4,128,75,126,null,103,null,110]
[7,"SSB-S9","CW 21.070,00","The higher, the more shown level",70,64.6,65,65,70,null,61,null,62]
[8,"SSB-FS","CW 21.070,00",null,62,56.6,57,56,62,null,54,null,54]
[9,"FM-S1","FM 145.375,00","60 = S0\nThe higher, the higher the S-value is",79,73,73,75,78,null,68,null,71]
[10,"FM-FS","FM 145.375,00",null,111,103.8,104,105,109,null,99,null,102]
[11,"DISC-L","FM 145.375,00","Press \"A\" at test signal given \"-3kHz\" and \"+3kHz\"",51,50.4,52,49,49,null,50,null,52]
[12,"DISC-H","FM 145.375,00",null,80,78,80,76,76,null,79,null,79]
[13,"FM-TH1","FM 145.375,00","open/close level\nwithout RX signal\n(Threshold / Hysteresis)",100,91.6,100,82,85,null,100,null,91]
[14,"FM-TH2","FM 145.375,00",null,101,92.6,101,88,86,null,100,null,88]
[15,"FM-TI1","FM 145.375,00","on RX signal of 3 dBµ\n(Tight = Enge)",6,4.4,6,1,3,null,10,null,2]
[16,"FM-TI2","FM 145.375,00",null,9,5.8,9,3,4,null,10,null,3]
[17,"VCC",null,"at Ub=13,8V",138,138,138,138,138,null,138,null,138]
[18,"HF1-IC","CW 1.825,07","the lower, the more sensitive the protection is",87,83.2,83,88,82,null,83,null,80]
[19,"HF2-IC","CW 7.043,55",null,87,82,82,86,82,null,80,null,80]
[20,"HF3-IC","CW 21.070,00",null,94,91,91,99,92,null,87,null,86]
[21,"50M-IC","CW 50.095,00",null,90,85.8,86,91,88,null,84,null,80]
[22,"VHF-IC","CW 145.375,00",null,79,71.6,72,72,73,null,72,null,69]
[23,"UHF-IC","CW 433.425,00",null,70,71.8,72,67,76,null,74,null,70]
[24,"HF1-MAX","CW 1.825,07","100W",174,165.6,166,163,167,null,165,null,167]
[25,"HF1-MID2","CW 1.825,07","50W",109,105.8,106,104,106,null,105,null,108]
[26,"HF1-MID1","CW 1.825,07","10W",34,31.2,31,31,30,null,31,null,33]
[27,"HF1-MIN","CW 1.825,07","5W",15,12.2,12,12,11,null,13,null,13]
[28,"HF2-MAX","CW 7.043,55","100W",168,160.2,160,158,163,null,159,null,161]
[29,"HF2-MID2","CW 7.043,55","50W",105,102.6,103,101,103,null,102,null,104]
[30,"HF2-MID1","CW 7.043,55","10W",32,29.6,30,29,29,null,29,null,31]
[31,"HF2-MIN","CW 7.043,55","5W",13,11.2,11,11,11,null,11,null,12]
[32,"HF3-MAX","CW 21.070,00","100W",167,159.2,159,156,162,null,158,null,161]
[33,"HF3-MID2","CW 21.070,00","50W",104,101.8,102,100,103,null,101,null,103]
[34,"HF3-MID1","CW 21.070,00","10W",32,29.2,29,29,28,null,29,null,31]
[35,"HF3-MIN","CW 21.070,00","5W",13,11.6,13,11,11,null,11,null,12]
[36,"50M-MAX","CW 50.095,00","100W",155,147.2,147,144,150,null,145,null,150]
[37,"50M-MID2","CW 50.095,00","50W",97,93,93,91,94,null,92,null,95]
[38,"50M-MID1","CW 50.095,00","10W",52,43.6,26,47,48,null,47,null,50]
[39,"50M-MIN","CW 50.095,00","5W",10,9.4,12,8,9,null,8,null,10]
[40,"VHF-PO-MAX","CW 145.375,00","50W",90,88.6,90,90,86,null,87,null,90]
[41,"VHF-PO-MID2","CW 145.375,00","20W",45,44.2,45,45,43,null,43,null,45]
[42,"VHF-PO-MIN","CW 145.375,00","5W",8,7.8,12,7,6,null,7,null,7]
[43,"UHF-PO-MAX","CW 433.425,00","20W",125,117.8,125,117,115,null,112,null,120]
[44,"UHF-PO-MIN","CW 433.425,00","5W",25,22.2,52,14,13,null,16,null,16]
[45,"HF1-TXG","USB 1.825,47","the higher, the higher the TX amplification of driver is (alignment that 5 W FM come out for sure)",64,53.4,60,71,47,null,48,null,41]
[46,"HF2-TXG","USB 7.043,55",null,64,43.4,60,47,38,null,38,null,34]
[47,"HF3-TXG","USB 21.070,00",null,64,49.6,60,63,44,null,43,null,38]
[48,"50MTXG","USB 50.095,00",null,64,44.8,60,50,39,null,40,null,35]
[49,"VHFTXG","USB 145.375,00",null,64,51.4,60,60,50,null,47,null,40]
[50,"UHFTXG","USB 433.425,00",null,64,56.2,60,49,49,null,49,null,74]
[51,"ALC1-M","USB 21.070,00","measured: 180\n-> value + 4 dots",250,171.8,205,246,0,null,203,null,205]
[52,"ALC-M","USB 21.070,00",null,100,90,100,98,82,null,85,null,85]
[53,"HF1-REV-ALC","CW 1.825,07","the lower, the more sensitive protection and reduction of output power",40,60,60,56,47,75,61,null,61]
[54,"HF2-REV-ALC","CW 7.043,55",null,36,55.333333333333336,55,49,42,75,56,null,55]
[55,"HF3-REV-ALC","CW 21.070,00",null,49,53,49,44,48,75,50,null,52]
[56,"50M-REV-ALC","CW 50.095,00",null,53,44.2,40,38,48,null,47,null,48]
[57,"VHF-REV-ALC","CW 145.375,00",null,57,65.8,90,57,61,null,62,null,59]
[58,"UHF-REV-ALC","CW 433.425,00",null,60,71.2,115,63,61,null,57,null,60]
[59,"CW-CAR-LEVEL","CW 21.070,00",null,109,145.2,145,148,144,null,144,null,145]
[60,"AM-CAR-LEVEL","AM 21.070,00","the lower the higher modulation level",114,127.4,125,134,125,null,125,null,128]
[61,"DEV-W","FM 145.375,00","deviation = 5 kHz",198,196.83333333333334,200,215,209,null,216,125,216]
[62,"DEV-N","FMN 145.375,00","deviation = 2.5 kHz",101,99.5,110,110,106,null,110,50,111]
[63,"MOD-MTR","FM 145.375,00","the lower, the more meter level",201,197.6,201,204,192,null,200,null,191]
[64,"DTMF-DEV","FM 145.375,00","the higher, the more deviation",10,31.2,10,46,47,null,10,null,43]
[65,"CTCSS-DEV","FM 145.375,00","the higher, the more deviation",235,223.16666666666666,235,246,225,null,233,160,240]
[66,"DCS-DEV","FM 145.375,00","the higher, the more\ndeviation",180,172.4,180,180,163,null,168,null,171]
[67,"LSB-CAR-POINT","LSB 21.070,00",null,0,-2.6,13,-8,-4,null,-7,null,-7]
[68,"USB-CAR-POINT","USB 21.070,00",null,0,0.2,-3,-5,0,null,5,null,4]
[69,"VSWR2 at 10W","CW 14.070,00",null,10,16.6,17,17,11,null,17,null,21]
[70,"VSWR3 at 10W","CW 14.070,00",null,32,41.4,44,44,32,null,42,null,45]
[71,"ATAS-TEST","LSB 14.070,00"]
[72,"AMTR-TEST","LSB 14.070,00"]
[73,"HTEMP-Threshold","LSB 14.070,00",null,null,38,38,38,38,null,38,null,38]
[74,"FTEMP-Threshold","LSB 14.070,00",null,null,102,102,102,102,null,102,null,102]
[{"$nulls":11},"Mic Gain"]
[null,"A+B+C (..or UP+Dn) + Power on  =  start alignment menu",{"$nulls":9},"FM = 15"]
[]
[null,"MEM/VFO CH  =  step through the menus"]
[]
[null,"MAIN DIAL  =  change value manually"]
[]
[null,"Power off  =  leave alignment menu WITHOUT STORING"]
[]
[null,"HOME  =  pre-setting factory defaults on each separate content  ---  see remarks (**)"]
[]
[null,"A  =  auto measuring of levels and storing them"]
[]
[null,"F  =  leave alignment menu WITH STORING ALL PARAMETERS  (1/2 sec.)"]
[]
[{"$nulls":8}," "]

{"sheet":"Internal Menu","index":1,"n_rows":48,"n_cols":9,"rows_kept":48,"cut":false,"hidden":false,"merged":[[0,5,0,8],[0,0,0,3]],"flags":["formulas_cached_only"]}
["FT-897 Menus",{"$nulls":4},"FT-897 Menus"]
["Menu #","Description","Settings","DG2IAQ Set",null,"Menu #","Description","Settings","DG2IAQ Set"]
["001","[EXT MENU] Enables or disables the extended menu mode.","ON / OFF","ON",null,"047","[DSP LPF CUTOFF] Adjust high-cut DSP LPF value","1000/1160/1320/1480/1650/1800/1970/2130/2290/2450/2610/2770/2940/3100/3260/3420/3580/3740/3900/4060/4230/4390/4550/4710/4870/5030/5190/5390/5520/5680/5840/6000 Hz","2770"]
["002","[144 MHz ARS] Toggle Auto Rpeater Shift for 2 meter FM repeater operation","ON / OFF",null,null,"048","[DSP MIC EQ] Sets DSP microphone equalization mode","OFF / LPF / HPF / BOTH"]
["003","[430 MHz ARS] Toggle Auto Repeater shift for 70cm FM repeater operation","ON / OFF",null,null,"049","[DSP NR LEVEL] Sets level of DSP Noise Reduction","1 ~ 16 (Def: 8)"]
["004","[AM & FM DIAL] Enable/Disable DIAL knob in AM and FM modes","ENABLE / DISABLE","ENABLE",null,"050","[EMERGENCY] Toggle Tx / Rx operation on 5167.5 kHZ (Alaska Emergency Channel)","ON / OFF"]
["005","[AM MIC GAIN] Adjust microphine gain in AM mode","0 ~ 100 (Def: 50)",null,null,"051","[FM MIC GAIN] Set microphone gain level in FM mode","0 ~ 100 (Def: 50)","9"]
["006","[AM STEP] Select tuning step for MEM/VFO CH knob in AM mode","2.5/5/9/10/12.5/25 kHZ","2.5",null,"052","[FM STEP] Set tuning step  for MEM / VFO / CH knob in FM","5 / 6.25 / 10 / 12.5 / 15 / 20 / 25 / 50 kHz","6.25"]
["007","[APO TIME] Select Auto Power Off time","OFF / 1Hr - 6Hrs",null,null,"053","[HOME-->VFO] Toggles moving HOME channel data to VFO","ON / OFF"]
["008","[ARTS BEEP] Select ARTS (Auto Range Transponder System) beep mode","ALL / RANGE / OFF (see manual for details)",null,null,"054","[LOCK MODE] Set function of LOCK key","DIAL / FREQ / PANEL / ALL"]
["009","[ARTS ID] Toggles CW Identifier during ARTS operation","ON / OFF","ON",null,"055","[MEM GROUP] Toggles memory grouping feature","ON / OFF"]
["010","[ARTS IDW] Store callsign into CW Identifier (up to 10 characters)","YAESU (see manual for details)","DG2IAQ 897",null,"056","[MEM TAG] Store Alphanumeric \"tags\" for memory channels","See manual for details"]
["011","[BEACON TEXT 1] Store Beacon message (up to 40 characters)","See Manual for details","DG2IAQ Beacon\n FT-897",null,"057","[MEM/VFO DIAL MODE] Sets  MEM / VFO CH knob function","Many available, see manual for details"]
["012","[BEACON TIME] Set Beacon interval","OFF / 1 ~ 255 sec.",null,null,"058","[MIC SCAN] Toggle scanning access via microphone [UP]/[DWN] Keys","ON / OFF"]
["013","[BEEP TONE] Select beep frequency","440 / 880 / 1760 Hz",null,null,"059","[MIC SEL] Sets controller type connected to Mic port","NOR / RMT / CAT"]
["014","[BEEP VOL] Sets Beep Volume","0 - 100 (Def: 50)","10",null,"060","[MTR ARX SEL] Selects meter type on Receive","SIG / CTR / VLT / N/A / FS / OFF"]
["015","[CAR LSB R] Set LSB Rx Carrier point","-300 ~ +300 Hz (Def: 0Hz)",null,null,"061","[MTR ATX SEL] Selects meter type on Transmit","PWR / ALC / SWR / MOD"]
["016","[CAR LSB T] Set LSB Tx Carrier point","-300 ~ +300 Hz (Def: 0Hz)",null,null,"062","[MTR PEAK HOLD] Toggles Peak Hold meter function ","ON / OFF"]
["017","[CAR USB R] Set USB Rx Carrier point","-300 ~ +300 Hz (Def: 0Hz)",null,null,"063","[NB LEVEL] Sets level of Noise Blanker","0 ~ 100 (Def: 50)","85"]
["018","[CAR USB T] Set USB Tx Carrier point","-300 ~ +300 Hz (Def: 0Hz)",null,null,"064","[OP FILTER1] Not Available",null,"FIL1"]
["019","[CAT RATE] Set CAT baud rate","4800 / 9600 / 38400 bps",null,null,"065","[PG A] Sets [A] key function in Multi-Function screen \"q\"","All MF functions avail. See Manual","MONI"]
["020","[CAT/LIN/TUN] Selects device connected to CAT/LINEAR jack","CAT / LINEAR / TUNER",null,null,"066","[PG B] Sets [B] key function in Multi-Function screen \"q\"","All MF functions avail. See Manual","Q.SPL"]
["021","[CLAR DIAL SEL] Sets knob to function as clarifier control","CLAR / M/V / MAIN",null,null,"067","[PG C] Sets [C] key function in Multi-Function screen \"q\"","All MF functions avail. See Manual","ATC"]
["022","[CW AUTO MODE] toggles KEY jack in SSB / AM / FM modes","ON / OFF",null,null,"068","[PG ACC] Not Available",null,"MONI"]
["023","[CW BFO] Set injection side of CW carrier oscillation","AUTO / LSB / USB",null,null,"069","[PG P1] Not Available",null,"Q.SPL"]
["024","[CW DELAY] Set Rx recovery time for semi-break-in CW operation","FULL / 30 - 3000 milliseconds (Def: 250ms)",null,null,"070","[PG P2] Not Available",null,"TCALL"]
["025","[CW KEY REV] Selects CW key wiring configuration","NORMAL / REVERSE",null,null,"071","[PKT 1200] Set audio input level for 1200 bps pakcet operation","0 ~ 100 (Def: 50)"]
["026","[CW PADDLE] Switch between ext. key and mic button keying","ELEKEY / MICKEY",null,null,"072","[PKT 9600] Set audio input level for 9600 bps pakcet operation","0 ~ 100 (Def: 50)"]
["027","[CW PITCH] Sets pitch of CW sidetone (steps of 50 Hz)","400 - 800 Hz (Def: 700 Hz)",null,null,"073","[PCKT RATE] Sets packet baud rate","1200 / 9600 bps"]
["028","[CW QSK] Set time delay between PTT and carrier Tx during QSK in CW mode","10 / 15 / 20 / 25 / 30 ms",null,null,"074","[PROC LEVEL] Sets level of the  speech processor (SSB / AM)","0 ~ 100 (Def: 50)","30"]
["029","[CW SIDETONE] Sets volume level of CW sidetone","0 ~ 100 (Def: 50)",null,null,"075","[RF POWER SET] Sets maximum power level for current band (in percentage)","5 ~ 100 ","5"]
["030","[CW SPEED] Set built-in keyer sending speed (In wpm or cpm, see maunual for details)","4wpm ~ 60wpm (Def: 12wpm)",null,null,"076","[RPT SHIFT] Sets repeater shift amount","0.00 ~ 99.99 MHz"]
["031","[CW TRAINING] Sets and enables CW Training feature","N / A / AN",null,null,"077","[SCAN MODE] Sets desired scan-resume mode","TIME / BUSY / STOP","TIME"]
["032","[CW WEIGHT] Sets built-in-keyer's Dot:Dash ratio","1:2.5 ~ 1:4.5 (Def: 1:3.0)",null,null,"078","[SCAN RESUME] Sets delay for scan resume when in TIME mode","1 ~ 10 sec.","5"]
["033","[DCS CODE] Sets DCS code (press MEM / VFO CH knob to toggle between ENCODE / DECODE)","104 standard DCS codes (Def: 023)","047",null,"079","[SPLIT TONE] Toggles split CTCSS / DCS coding","ON / OFF"]
["034","[DCS INV] Select NORMAL or INVERTED DCS coding","Tn-Rn / Tn-Riv / Tiv-Rn / Tiv-Riv ",null,null,"080","[SQL RF GAIN] Sets function of SQL / RF knob","RF-GAIN / SQL","SQL"]
["035","[DIAL STEP] Sets speed of main DIAL","FINE / COARSE",null,null,"081","[SSB MIC GAIN] adjusts Microphone gain on SSB","0 ~ 100 (Def: 50)","75"]
["036","[DIG DSP] Set displayed frequency offset in DIGITAL mode","-3000 ~ +3000 Hz (Def: 0Hz)",null,null,"082","[SSB STEP] Sets tuning steps for MEM / VFO CH knob in SSB","1 / 2.5 / 5 kHZ"]
["037","[DIG GAIN] Sets audio input level used during DIGITAL mode ","0 ~ 100 (Def: 50)",null,null,"083","[TONE FREQ] Sets CTCSS tone frequency","50 standard CTCSS tones (Def: 88.5Hz)"]
["038","[DIG MODE] Set mode and sideband for DIGITAL mode operation","RTTY-L / RTTY-U */ PSK31-L / PSK31-U / USER-L / USER-U      *see manual details",null,null,"084","[TOT TIME] Sets value for Time Out Timer","OFF / 1m ~ 20m","3m"]
["039","[DIG SHIFT] Set carrier freq offset during DIGITAL (USER-L or USER-U) mode operation","-3000 ~ +3000 Hz (Def: 0Hz)",null,null,"085","[TUNER / ATAS] Sets device to control for the [TUN] key (MF row \"k\" button [A] )","OFF / ATAS(HF) / ATAS(HF&50) / ATAS(ALL) / TUNER"]
["040","[DIG VOX] Sets input level for DIGITAL mode","0 ~ 100 (Def: 50)",null,null,"086","[TX IF FILTER] Selects TX IF filter","CFIL / OPF1 / OPF2","CFIL"]
["041","[DISP COLOR] Sets display color for each operating status","0 ~ 32","ARTS: 1",null,"087","[VOX DELAY] Sets hang time for VOX operation","100 ~ 300 ms","800"]
["042","[DISP CONTRAST] Sets the display contrast level","1 ~ 15 (Def: 5)","5",null,"088","[VOX GAIN] Sets sensitivity of VOX input audio detector","1 ~ 100 (Def: 50)"]
["043","[DISP INTENSITY] Sets display brightness level","0 (DIM) ~ 2 (BRIGHT)","2",null,"089","[XVTR A FREQ] Sets IF of first transverter (if installed)","Arbitrary"]
["044","[DISP MODE] Sets LCD Lamp mode","OFF / AUTO1 / AUTO2 / ON",null,null,"090","[XVTR B FREQ] Sets IF of second transverter (if installed)","Arbitrary"]
["045","[DSP BPF WIDTH] Sets bandwidth for the DSP CW audio filter","60 / 120 / 240 Hz",null,null,"091","[XVTR SEL] Selects antenna port used for transverter operation","OFF / XVTR A / XVTR B"]
["046","[DSP HPF CUTOFF] Adjust the low-cut DSP HPF value","100/160/220/280/340/400/460/520/580/640/700/760/820/880/940/1.000 Hz","220"]